|  |
| --- |
| “Grid pitch…” command |
| **Purpose**  **“Grid pitch...”** command is intended for simplifying the process of drawing, mutual alignment of graphic objects and for arrangement of units in the diagram window. |
| To activate the command select **“Grid pitch…”** command in **“View”** tab of **Diagram window**.  On activation of **“Grid pitch…”** command, a dialog window to enter a required grid pitch value will appear on top of **Diagram window**.    Press **“OK”** key to confirm the command and set a new grid pitch.  The user also can disable the visibility of grid using **“Grid”** switch in **“View”** menu item of **Diagram window.**  **Recommendation for application in the process of work:**  Grid pitch shall be set prior to creation of a project and it is not recommended to change it in the process of creation to make the project look neat and tidy.  In the process of creation of a project it is allowable to change the grid pitch for a multiple one, e.g., from 8 pt to 4 pt for drawing finer details and then to return back to 8 pt.  In the process of zoom-in (-out) of the project, snap can be done not only for grid points but also for passing points. |